Glareshield

PANEL

PITOT

Fuel Transfer

AVIO

VS -

VS +

VS

Cursor

Cursor

INNER

OUTER

AP

TAXI

ALT

FD

FLC+

FLC-

MFD INNER

MFD OUTER

FLC

POSITION

CRS 2

RANGE

BARO 2

BARO

SWAP

1/2

ACTIVE

/STBY

CRS 1

set

NAV

KHz

ALT 100

ALT 1000

MHz

KHz

HDG

MHz

CRS 1

COM

HDG

SET

SWAP

1/2

ACTIVE

/STBY

BEST FLC

BC

VNAV

APR

NAV 1

HDG HOLD

DA40 - TDI

GPS

XPNDR

MHz

KHz

OUTER

INNER

OBS1

BAR

C Swap

V Swap

CDI

OBS

MSG

FLP

PROC

DRIFT

Off

ON

STBY

ALT

VFR

IDENT

TEST

0

1

2

3

4

5

6

7

RNG out

RNG in

DIR

CLR

ENT

RANGE

CURSOR

FLOOD

On/OFF

ISNT on/off

C/V

SWAP

Com/NAV

AP

GPS and LIGHTS

MENU

CLR

CABIN

FLP

DIR

Strobe

LAND

VOR 2

FMS

ENT

PROC

DA40 NG

MENU

INST

FLOOD